T-Index

Summary:
- A
- B
- C
- D
- E
- F
- G
- H
- I
- J
- K
- L
- M
- N
- O
- P
- Q
- R
- S
- T
- U
- V
- W

##
T

TIMEOUT_BETWEEN_SAME_SYMBOL

- Static variable in class android.device.scanner.configuration. PropertyID
  To set Scanner decoding timeout between same symbol Parameters Values: value * 100 ms VALUE_TIMEOUT_BETWEEN_SAME_SYMBOL_min 1 VALUE_TIMEOUT_BETWEEN_SAME_SYMBOL_max 99 VALUE_TIMEOUT_BETWEEN_SAME_SYMBOL_Default 10

toInt()

- Method in enum android.device.scanner.configuration. Symbology
  Converts the Symbology to its corresponding integer value.

toInt()

- Method in enum android.device.scanner.configuration. Triggering

Triggering

- Enum in android.device.scanner.configuration
  Trigger decode Mode
  CONTINUOUS A trigger pull activates the laser and decode processing.

TRIGGERING_LOCK

- Static variable in class android.device.scanner.configuration. PropertyID

TRIGGERING_MODES

- Static variable in class android.device.scanner.configuration. PropertyID
  To set Scanner trigger modes Parameters Values: `Triggering`

TRIOPTIC

- Static variable in class android.device.scanner.configuration. Constants.Symbology

TRIOPTIC_ENABLE

- Static variable in class android.device.scanner.configuration. PropertyID

type

- Variable in class android.device. KeyMapManager.KeyEntry
  Describes `KeyMapManager.KEY_TYPE_KEYCODE` or `KeyMapManager.KEY_TYPE_STARTAC`