I-Index

Summary:
- A
- B
- C
- D
- E
- F
- G
- H
- I
- J
- K
- L
- M
- N
- O
- P
- Q
- R
- S
- T
- U
- V
- W

##
I

I25_ENABLE

- Static variable in class android.device.scanner.configuration.PropertyID

I25_ENABLE_CHECK

- Static variable in class android.device.scanner.configuration.PropertyID

I25_LENGTH1

- Static variable in class android.device.scanner.configuration.PropertyID

I25_LENGTH2

- Static variable in class android.device.scanner.configuration.PropertyID

I25_SEND_CHECK

- Static variable in class android.device.scanner.configuration.PropertyID

I25_TO_EAN13

- Static variable in class android.device.scanner.configuration.PropertyID

IccManager

- Class in android.device
  The IccManager class is used to initialize and control the smart card reader, to sends a command Application Protocol Data Unit(APDU) to a card and retrieve the response APDU.

IccManager()

- Constructor for class android.device.IccManager

idcard_apduTransmit(byte[], int, byte[])

- Method in class android.device.PiccManager
  Transmit APDU commands

idcard_init()

- Method in class android.device.PiccManager
  init the IDCARD

IMAGE_EXPOSURE_MODE

- Static variable in class android.device.scanner.configuration.PropertyID

IMAGE_FIXED_EXPOSURE

- Static variable in class android.device.scanner.configuration.PropertyID

IMAGE_ONE_D_INVERSE

- Static variable in class android.device.scanner.configuration.PropertyID
  IMAGE_ONE_D_INVERSE: REGULAR_ONLY = 0; INVERSE_ONLY = 1; INVERSE_AUTOD = 2;

IMAGE_PICKLIST_MODE

- Static variable in class android.device.scanner.configuration.PropertyID
  To set 2D Scanner phone modes Parameters Values: VALUE_IMAGE_PICKLIST_MODE_Enable 1 VALUE_IMAGE_PICKLIST_MODE_Disable 0 VALUE_IMAGE_PICKLIST_MODE_Default 0

INTERLEAVED25

- Static variable in class android.device.scanner.configuration.Constants.Symbology

isInterception()

- Method in class android.device.KeyMapManager
  Returns true if enable system remap Button key event.

isSymbologyEnabled(Symbology)

- Method in class android.device.ScanManager
  Returns current enable setting for a particular barcode symbology.

isSymbologySupported(Symbology)

- Method in class android.device.ScanManager
  Return true if the device's decoder is able to read a particular barcode symbology.