M-Index

Summary:
- A
- B
- C
- D
- E
- F
- G
- H
- I
- J
- K
- L
- M
- N
- O
- P
- Q
- R
- S
- T
- U
- V
- W

##
M

m1_amount(int)

- Method in class android.device.PiccManager
  read the amount for the block number

m1_decrement(int, int)

- Method in class android.device.PiccManager
  decrement the value block by iMoney amount

m1_increment(int, int)

- Method in class android.device.PiccManager
  increment the value block by iMoney amount

m1_init(int, int)

- Method in class android.device.PiccManager
  init the value block by value

m1_keyAuth(int, int, int, byte[], int, byte[])

- Method in class android.device.PiccManager
  authenticate a key

m1_readBlock(int, byte[])

- Method in class android.device.PiccManager
  To read a block

m1_restore(int)

- Method in class android.device.PiccManager
  Move the content of a block into temporary data register

m1_transfer(int)

- Method in class android.device.PiccManager
  transfer from temporary internal data register to value block

m1_writeBlock(int, int, byte[])

- Method in class android.device.PiccManager
  Write a block into the card

M25_ENABLE

- Static variable in class android.device.scanner.configuration.PropertyID

MagManager

- Class in android.device
  The MagManager class is used to initialize and control the MSR card reader.

MagManager()

- Constructor for class android.device.MagManager

mapKeyEntry(KeyEvent, int, String)

- Method in class android.device.KeyMapManager
  Create a new key event remap that is the same as the given one, but whose keycode is replaced with the given value.

MATRIX25

- Static variable in class android.device.scanner.configuration.Constants.Symbology

MAXICODE

- Static variable in class android.device.scanner.configuration.Constants.Symbology

MAXICODE_ENABLE

- Static variable in class android.device.scanner.configuration.PropertyID

MICROPDF417

- Static variable in class android.device.scanner.configuration.Constants.Symbology

MICROPDF417_ENABLE

- Static variable in class android.device.scanner.configuration.PropertyID

MICROQRCODE_ENABLE

- Static variable in class android.device.scanner.configuration.PropertyID

MSI

- Static variable in class android.device.scanner.configuration.Constants.Symbology

MSI_CHECK_2_MOD_11

- Static variable in class android.device.scanner.configuration.PropertyID

MSI_ENABLE

- Static variable in class android.device.scanner.configuration.PropertyID

MSI_LENGTH1

- Static variable in class android.device.scanner.configuration.PropertyID

MSI_LENGTH2

- Static variable in class android.device.scanner.configuration.PropertyID

MSI_REQUIRE_2_CHECK

- Static variable in class android.device.scanner.configuration.PropertyID

MSI_SEND_CHECK

- Static variable in class android.device.scanner.configuration.PropertyID

MULTI_DECODE_MODE

- Static variable in class android.device.scanner.configuration.PropertyID