G-Index

Summary:
- A
- B
- C
- D
- E
- F
- G
- H
- I
- J
- K
- L
- M
- N
- O
- P
- Q
- R
- S
- T
- U
- V
- W

##
G

generateRandomData(byte[], byte[])

- Method in class android.device.SEManager
  Generate a 8 bytes random number.

getAllStripInfo(byte[])

- Method in class android.device.MagManager
  Get information on all 3 strips

getDeviceId()

- Method in class android.device.DeviceManager
  Get the device product serial number

getDockerState()

- Method in class android.device.DeviceManager
  Support i9000S(Android 4.3/Android5.1) only.Return the currently active docking station connected state .

getEncryptStripInfo(int, int, byte[], byte[], byte[])

- Method in class android.device.MagManager
  Get information on all 3 Encrypt strips data and plain text card NO.

getFirmwareVersion(byte[], byte[])

- Method in class android.device.SEManager
  get security processor firmware version.

getKeyAction(int)

- Method in class android.device.KeyMapManager
  Returns special actions if this scan code is a KeyEvent keycode.

getKeyCode(int)

- Method in class android.device.KeyMapManager
  Returns new keycode if this scan code is a KeyEvent keycode.

getKeyList()

- Method in class android.device.KeyMapManager
  Returns all remap keys describes.

getKeyMeta(int)

- Method in class android.device.KeyMapManager

getKeytype(int)

- Method in class android.device.KeyMapManager
  Returns ramap type if this scan code is a KeyEvent keycode.

getOutputMode()

- Method in class android.device.ScanManager
  get current the scan result output mode

getParameterInts(int[])

- Method in class android.device.ScanManager
  Gets one or more programming parameters of type Integer from the scan engine

getParameterString(int[])

- Method in class android.device.ScanManager
  Gets label programming parameters of type String at the specified indexs.

getPinBlock(int, int, byte[], int, String, long, SEManager.PedInputListener)

- Method in class android.device.SEManager
  Get the pin block.

getPinBlockEx(int, int, byte[], int, String, long, String, SEManager.PedInputListener)

- Method in class android.device.SEManager
  Get the pin block.

getPinBlockEx(android.os.Bundle, SEManager.PedInputListener)

- Method in class android.device.SEManager
  Get the pin block.

getResponseEnable(byte)

- Method in class android.device.IccManager
  Set whether the drive layer to the 61xx, 6Cxx and other commands for automatic data acquisition, the default for automatic acquisition.

getScannerState()

- Method in class android.device.ScanManager
  get the scanner power states

getSingleStripInfo(int, byte[])

- Method in class android.device.MagManager
  Get specific strip information

getStatus()

- Method in class android.device.PrinterManager
  Gets the current state of the printer `PrinterManager.PRNSTS_OK` `PrinterManager.PRNSTS_OUT_OF_PAPER` `PrinterManager.PRNSTS_OVER_HEAT` `PrinterManager.PRNSTS_UNDER_VOLTAGE` `PrinterManager.PRNSTS_BUSY` `PrinterManager.PRNSTS_ERR` `PrinterManager.PRNSTS_ERR_DRIVER` Returns the printer status. 0 for status OK

getStatus(byte[], byte[])

- Method in class android.device.SEManager
  get security processor hardware status

getTIDSN()

- Method in class android.device.DeviceManager

getTriggerLockState()

- Method in class android.device.ScanManager
  get the scan trigger status

getTriggerMode()

- Method in class android.device.ScanManager
  Returns current configure triggering decode mode.

GOOD_READ_BEEP_ENABLE

- Static variable in class android.device.scanner.configuration.PropertyID

GOOD_READ_VIBRATE_ENABLE

- Static variable in class android.device.scanner.configuration.PropertyID

GS1_128

- Static variable in class android.device.scanner.configuration.Constants.Symbology

GS1_14

- Static variable in class android.device.scanner.configuration.Constants.Symbology

GS1_14_ENABLE

- Static variable in class android.device.scanner.configuration.PropertyID

GS1_14_TO_UPC_EAN

- Static variable in class android.device.scanner.configuration.PropertyID

GS1_EXP

- Static variable in class android.device.scanner.configuration.Constants.Symbology

GS1_EXP_ENABLE

- Static variable in class android.device.scanner.configuration.PropertyID

GS1_EXP_LENGTH1

- Static variable in class android.device.scanner.configuration.PropertyID

GS1_EXP_LENGTH2

- Static variable in class android.device.scanner.configuration.PropertyID

GS1_LIMIT

- Static variable in class android.device.scanner.configuration.Constants.Symbology

GS1_LIMIT_ENABLE

- Static variable in class android.device.scanner.configuration.PropertyID