Triggering

## android.device.scanner.configuration
Enum Triggering

    java.lang.Object
      java.lang.Enum<Triggering>
          android.device.scanner.configuration.Triggering

All Implemented Interfaces:
  java.io.Serializable, java.lang.Comparable<Triggering>

    public enum Triggering

extends java.lang.Enum<Triggering>

Trigger decode Mode:

PULSE | Automatic mode. After the scan is triggered, the light is decoded until the valid barcode is scanned or the laser is turned on and timed out.
CONTINUOUS | Continuous mode. After the scan is triggered, the light is decoded, and it ends after scanning to a valid barcode or after the laser is turned on, and then starts the next scan.
HOST | Manual mode. A host command issues the triggering signal, the scan engine interprets an actual trigger pull as a Level triggering option.

Enum Constant Summary
`PULSE` Automatic mode. After the scan is triggered, the light is decoded until the valid barcode is scanned or the laser is turned on and timed out.
`CONTINUOUS` Continuous mode. After the scan is triggered, the light is decoded, and it ends after scanning to a valid barcode or after the laser is turned on, and then starts the next scan.
`HOST` Manual mode. A host command issues the triggering signal, the scan engine interprets an actual trigger pull as a Level triggering option.

Method Summary
`int` | `toInt()` Convert the Triggering to its corresponding integer value.
`static Triggering` | `valueOf(java.lang.String name)` Return the enum constant of this type with the specified name.
`static Triggering[]` | `values()` Return an array containing the constants of this enum type, in the order they are declared.

Methods inherited from class java.lang.Enum
`compareTo, equals, getDeclaringClass, hashCode, name, ordinal, toString, valueOf`

Methods inherited from class java.lang.Object
`getClass, notify, notifyAll, wait, wait, wait`

Enum Constant Detail

### PULSE

    public static final Triggering PULSE

  Automatic mode. After the scan is triggered, the light is decoded until the valid barcode is scanned or the laser is turned on and timed out.

### CONTINUOUS

    public static final Triggering CONTINUOUS

  Continuous mode. After the scan is triggered, the light is decoded, and it ends after scanning to a valid barcode or after the laser is turned on, and then starts the next scan.

### HOST

    public static final Triggering HOST

  Manual mode. A host command issues the triggering signal, the scan engine interprets an actual trigger pull as a Level triggering option.

Method Detail

### values

    public static Triggering[] values()

  Returns an array containing the constants of this enum type, in the order they are declared. This method may be used to iterate over the constants as follows:

  Parameters:
    none
  Returns:
    an array containing the constants of this enum type, in the order they are declared.
  Example:
    `for (Triggering c : Triggering.values())
    System.out.println(c);`

### valueOf

    public static Triggering valueOf(java.lang.String name)

  Returns the enum constant of this type with the specified name. The string must match exactly an identifier used to declare an enum constant in this type. (Extraneous whitespace characters are not permitted.)

  Parameters:
    `name` - The name of the enum constant to be returned.
  Returns:
    the enum constant with the specified name.
  Throws:
    `java.lang.IllegalArgumentException` - if this enum type has no constant with the specified name
    `java.lang.NullPointerException` - if the argument is null

### toInt

    public int toInt()

  Converts the Triggering to its corresponding integer value.
  Parameters:
    none
  Returns:
    int representing a Triggering value.