A-Index

Summary:
- A
- B
- C
- D
- E
- F
- G
- H
- I
- J
- K
- L
- M
- N
- O
- P
- Q
- R
- S
- T
- U
- V
- W

##
A

action

- Variable in class android.device. KeyMapManager.KeyEntry
  Describes the special actions to start APPS `android.content.Intent`

ACTION_DECODE

- Static variable in class android.device. ScanManager

activate(byte[])

- Method in class android.device. IccManager
  Activate and reset the card

activate()

- Method in class android.device. PiccManager
  activate card to start sending APDU。

activateEx(byte[])

- Method in class android.device. PiccManager
  activate card to start sending APDU。

android.device

- package android.device

android.device.scanner.configuration

- package android.device.scanner.configuration

antisel(byte[], byte[])

- Method in class android.device. PiccManager
  anti-collision and select card and returns the serial number of the card

apduTransmit(byte[], int, byte[], byte[])

- Method in class android.device. IccManager
  Transmit APDU to the IC card

apduTransmit(byte[], int, byte[], byte[])

- Method in class android.device. PiccManager
  Transmit APDU commands

apduTransmit(byte[], int, byte[])

- Method in class android.device. PiccManager
  Transmit APDU exchange commands:e.g.

apduTransmit(byte[], int, byte[], int, int)

- Method in class android.device. PiccManager
  Transmit APDU exchange commands:e.g.

apduTransmit(int, int, byte[], int, byte[])

- Method in class android.device. PiccManager
  Transmit APDU commands for F Card

at88sc102_read(int, int)

- Method in class android.device. IccManager
  Read the data stored in main memory for At88sc102

at88sc102_VerifyPassword(int, byte[], int)

- Method in class android.device. IccManager
  Check & Verify password for At88sc102.

at88sc102_write(int, byte[], int)

- Method in class android.device. IccManager
  Write data to the main storage area At88sc102

AUSTRALIAN_POST_ENABLE

- Static variable in class android.device.scanner.configuration. PropertyID

AZTEC

- Static variable in class android.device.scanner.configuration. Constants.Symbology

AZTEC_ENABLE

- Static variable in class android.device.scanner.configuration. PropertyID

AZTEC_INVERSE

- Static variable in class android.device.scanner.configuration. PropertyID