S-Index

Summary:
- A
- B
- C
- D
- E
- F
- G
- H
- I
- J
- K
- L
- M
- N
- O
- P
- Q
- R
- S
- T
- U
- V
- W

##
S

S_OK

- Static variable in class android.device.SEManager
  command execute Success

scancode

- Variable in class android.device.KeyMapManager.KeyEntry
  Describes the Button event scan code`android.view.KeyEvent#getScanCode()`

ScanManager

- Class in android.device
  The ScanManager class provides developers access to barcode reader related in the device To decode bar codes with this class, use the following steps: Obtain an instance of BarCodeReader with ScanManager scan = new ScanManager().

ScanManager()

- Constructor for class android.device.ScanManager

SEManager

- Class in android.device
  The SEManager class is used to initialize and control the security processor hardware To control the security processor hardware with this class, use the following steps: You can obtain an instance of this class by calling.

SEManager()

- Constructor for class android.device.SEManager

SEManager.OperationPedInputListener

- Interface in android.device
  The application has to implement the appropriate listener

SEManager.PedInputListener

- Interface in android.device

SEND_GOOD_READ_BEEP_ENABLE

- Static variable in class android.device.scanner.configuration.PropertyID
  To set Scanner success beep or vibrate when SendBroadcast SendBroadcast Values: `WEDGE_INTENT_ACTION_NAME` `WEDGE_INTENT_DATA_STRING_TAG`

SEND_GOOD_READ_VIBRATE_ENABLE

- Static variable in class android.device.scanner.configuration.PropertyID

SEND_LABEL_PREFIX_SUFFIX

- Static variable in class android.device.scanner.configuration.PropertyID

setAPN(String, String, String, int, String, String, String, String, String, String, String, int, int, String, String, int, String, boolean)

- Method in class android.device.DeviceManager
  Sets the APN (access point name) configurations for mobile data network

setCurrentTime(long)

- Method in class android.device.DeviceManager
  Sets the current wall time, in milliseconds.

setETU(int)

- Method in class android.device.IccManager
  Set the ETU.

setGrayLevel(int)

- Method in class android.device.PrinterManager
  Set print gray level

setParameterInts(int[], int[])

- Method in class android.device.ScanManager
  Sets one or more label programming parameters of type Int

setParameterString(int[], String[])

- Method in class android.device.ScanManager
  Set the scanner parameter of type String at the specified indexes.

setSpeedLevel(int)

- Method in class android.device.PrinterManager
  Set print speed level

setSuspendTimeout(int, byte[], byte[])

- Method in class android.device.SEManager
  This function allows to set the security processor timeout before automatic suspension.

setTriggerMode(Triggering)

- Method in class android.device.ScanManager
  This method set specifies which mode to control decode.

setupPage(int, int)

- Method in class android.device.PrinterManager
  Set the page size.

sle4428_password(int, byte[])

- Method in class android.device.IccManager
  Submit the transfer data, enter the personalization mode

sle4428_readMemory(int, int)

- Method in class android.device.IccManager
  Read the data stored in main memory for SLE4428

sle4428_reset(byte[])

- Method in class android.device.IccManager
  reset the SLE4428

sle4428_writeMemory(int, byte[], int)

- Method in class android.device.IccManager
  Write data to the main storage area SLE4428

sle4436_authenticate(int, byte[], byte[])

- Method in class android.device.IccManager
  Get the Card verification certificate

sle4436_decValue(int)

- Method in class android.device.IccManager
  Reduction balance

sle4436_readBit(byte[])

- Method in class android.device.IccManager
  Read values from the Card bit

sle4436_readMemory(int, int)

- Method in class android.device.IccManager
  Read the data stored in main memory for SLE4436

sle4436_regIncrease(int)

- Method in class android.device.IccManager
  Move the register

sle4436_reloadByte()

- Method in class android.device.IccManager
  Reload Byte

sle4436_reset(byte[])

- Method in class android.device.IccManager
  reset the SLE4436

sle4436_verifyPassword(byte[])

- Method in class android.device.IccManager
  Submit the transfer data, enter the personalization mode

sle4436_writeBit()

- Method in class android.device.IccManager
  Write a byte for Card

sle4436_writeCarry(int, int, byte[], int)

- Method in class android.device.IccManager
  Write Carry data

sle4436_writeMemory(int, byte[], int)

- Method in class android.device.IccManager
  Write data to the main storage area SLE4436

sle4442_changePassword(byte[])

- Method in class android.device.IccManager
  Change password.

sle4442_readErrorCounter(byte[])

- Method in class android.device.IccManager
  Change password.

sle4442_readMainMemory(int, int)

- Method in class android.device.IccManager
  Read the data stored in main memory for SLE4442

sle4442_readProtectionMemory(int, int)

- Method in class android.device.IccManager
  Read SLE4442 card protection bit storage data (4 BYTE). 4 bytes of data read is to save the SLE4442 bits data in storage area.

sle4442_reset(byte[])

- Method in class android.device.IccManager
  reset the SLE4442

sle4442_verifyPassword(byte[])

- Method in class android.device.IccManager
  Comparison of SLE4442 cards, each card after power compared to the card password, otherwise the card data is read-only, you will not be on the card of any write operation.

sle4442_writeMainMemory(int, byte[], int)

- Method in class android.device.IccManager
  Write data to the main storage area SLE4442

sle4442_writeProtectionMemory(int, byte[], int)

- Method in class android.device.IccManager
  The write protection bit storage area.

startDecode()

- Method in class android.device.ScanManager
  Call this method to start decoding.

stopDecode()

- Method in class android.device.ScanManager
  This stops any data acquisition currently in progress.

switchOutputMode(int)

- Method in class android.device.ScanManager
  Use this function to set the output mode of the barcode reader (either send output to text box or as Android intent).

Symbology

- Enum in android.device.scanner.configuration
  `Symbology` is an enumeration class defining constants for different barcode types.