PropertyID

## android.device.scanner.configuration
Class PropertyID

    java.lang.Object
      android.device.scanner.configuration.PropertyID

    public final class PropertyID

extends java.lang.Object

Field Summary
`static int` | `AUSTRALIAN_POST_ENABLE` This property specifies whether Australia Post decoding is enabled.
`static int` | `AZTEC_ENABLE` This property specifies whether Aztec Code decoding is enabled.
`static int` | `AZTEC_INVERSE` Set the Aztec inverse decoder setting: Regular Only/ Inverse Only/ Inverse Autodetect. Note: The parameter values below are ONLY supported on platforms interfacing to the Zebra Technologies imagers.
`static int` | `C25_ENABLE` This property specifies whether chinese 2 of 5 post decoding is enabled.
`static int` | `CODABAR_CLSI` Enable this parameter to strip the start and stop characters and insert a space after the first, fifth, and tenth characters of a 14-character Codabar symbol.
`static int` | `CODABAR_ENABLE` This property specifies whether Codabar decoding is enabled.
`static int` | `CODABAR_ENABLE_CHECK` This property specifies whether Codabar check digit verification is enable.
`static int` | `CODABAR_LENGTH1` Set minimun length for Codabar. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `CODABAR_LENGTH2` Set maximun length for Codabar. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `CODABAR_NOTIS` Enable this parameter to strip the start and stop characters from a decoded Codabar symbol.
`static int` | `CODABAR_SEND_CHECK` This property specifies whetherto transmit Codabar data with or without the check digit.
`static int` | `CODABAR_SEND_START` Start/Stop characters identify the leading and trailing ends of the bar code.
`static int` | `CODE_ISBT_128` ISBT 128 is a variant of Code128 used in the blood bank industry.
`static int` | `CODE_ISBT_Concatenation_MODE` Select an option for concatenating pairs of ISBT code types: 0 : Disable ISBT Concatenation - The device does not concatenate pairs of ISBT codes it encounters.
`static int` | `CODE11_ENABLE` This property specifies whether Codes11 decoding is enabled.
`static int` | `CODE11_ENABLE_CHECK` This feature allows the decoder to check the integrity of all Code11 symbols to verify that the data complies with the specified check digit algorithm.
`static int` | `CODE11_LENGTH1` Set minimun length for Code11. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `CODE11_LENGTH2` Set maximun length for Code11. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `CODE11_SEND_CHECK` This property specifies whether or not to transmit the Code11 check digit(s).
`static int` | `CODE128_CHECK_ISBT_TABLE` The ISBT specification includes a table that lists several types of ISBT bar codes that are commonly used in pairs.
`static int` | `CODE128_ENABLE` This property specifies whether Code128 decoding is enabled.
`static int` | `CODE128_GS1_ENABLE` This property specifies whether GS1-128 decoding is enabled.
`static int` | `CODE128_IGNORE_FNC4` This feature applies to Code128 bar codes with an embedded character. 0 : Disable Ignore Code128; The character is not transmitted but the following character has 128 added to it. 1 : Enable Ignore Code128; This strips the character from the decode data. The remaining characters do not change.
`static int` | `CODE128_LENGTH1` Set minimun length for Code128. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `CODE128_LENGTH2` Set maximun length for Code128. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `CODE128_REDUCED_QUIET_ZONE` Enable or disable decoding Code128 bar codes with reduced quiet zones. The property value should be set as follows: 0 : Disallow short quiet zone symbols.
`static int` | `CODE128_SECURITY_LEVEL` Code128 bar codes are vulnerable to misdecodes, particularly when Code128 Lengths is set to Any Length.
`static int` | `CODE32_ENABLE` This property specifies whether Code32 decoding is enabled.
`static int` | `CODE32_SEND_START` Enable or disable adding the prefix character “A” to all Code32 bar codes.
`static int` | `CODE39_ENABLE` This property specifies whether Code39 decoding is enabled.
`static int` | `CODE39_ENABLE_CHECK` Enable this to check the integrity of all Code39 symbols to verify that the data complies with specified check digit algorithm.
`static int` | `CODE39_FULL_ASCII` Code39 Full ASCII is a variant of Code39 which pairs characters to encode the full ASCII character set.
`static int` | `CODE39_LENGTH1` Set minimun length for Code39. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `CODE39_LENGTH2` Set maximun length for Code39. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `CODE39_Quiet_Zone` Enable or disable decoding Code39 bar codes with reduced quiet zones.
`static int` | `CODE39_SECURITY_LEVEL` The scanner offers four levels of decode security for Code39 barcodes.
`static int` | `CODE39_SEND_CHECK` This property specifies whether to transmit Code39 data with or without the check digit.
`static int` | `CODE39_START_STOP` Start/Stop characters identify the leading and trailing ends of the bar code.
`static int` | `CODE93_ENABLE` This property specifies whether Codabar decoding is enabled.
`static int` | `CODE93_LENGTH1` Set minimun length for Code39. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `CODE93_LENGTH2` Set maximun length for Code39. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `CODING_FORMAT` This property specifies the character encoding to use for the bar code data.
`static int` | `COMPOSITE_CC_AB_ENABLE` This property specifies whether Composite CC-A/B decoding is enabled.
`static int` | `COMPOSITE_CC_C_ENABLE` This property specifies whether Composite CC-C decoding is enabled.
`static int` | `COMPOSITE_TLC39_ENABLE` This property specifies whether Composite TLC-39 decoding is enabled.
`static int` | `D25_ENABLE` This property specifies whether Discrete 2 of 5 decoding is enabled.
`static int` | `D25_LENGTH1` Set minimun length for Discrete 2 of 5. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `D25_LENGTH2` Set maximun length for Discrete 2 of 5. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `DATAMATRIX_ENABLE` This property specifies whether DataMatrix decoding is enabled.
`static int` | `DATAMATRIX_INVERSE` Set the DATAMATRIX inverse decoder setting: Regular Only/ Inverse Only/ Inverse Autodetect. Note: The parameter values below are only supported on platforms interfacing to the Zebra Technologies imagers.
`static int` | `DATAMATRIX_LENGTH1` Set minimun length for DataMatrix. Range: 1 to 3166. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `DATAMATRIX_LENGTH2` Set minimun length for DataMatrix. Range: 1 to 3166. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `DEC_2D_CENTERING_ENABLE` This property specifies whether Centering mode decoding is enabled.
`static int` | `DEC_2D_CENTERING_MODE` Mode Configuration settings:Off/Around Aimer/Field Of View. Note: The parameter values below are ONLY supported on platforms interfacing to the Honeywell 6703/6603 scanner.
`static int` | `DEC_2D_LIGHTS_MODE` This property specifies whether the lights mode settings. Lights Configuration settings:(Illum/Aimer Off)/(Aimer Only)/(Illum Only)/(Alternating)/(Concurrent).
`static int` | `DEC_2D_WINDOW_LOWER_RX` Upper right X coordinate setting : default 386, min 0, max 415.
`static int` | `DEC_2D_WINDOW_LOWER_RY` Upper right Y coordinate setting : default 446, min 416, max 831.
`static int` | `DEC_2D_WINDOW_UPPER_LX` Upper left X coordinate setting : default 290, min 0, max 319.
`static int` | `DEC_2D_WINDOW_UPPER_LY` Upper left Y coordinate setting :default 350, min 320, max 639.
`static int` | `DEC_ES_CONFORM_IMAGE` The image must conform to the auto-exposure requirements, if not, it's rejected. Valid Values: Rang 0to 1.
`static int` | `DEC_ES_CONFORM_TRIES` The number of time it will attempt to conform Valid Values: Rang 1 to 8.
`static int` | `DEC_ES_FIXED_FRAME_RATE` If exposure mode is FIXED, what is the frame rate (fixed, has no effect) Valid Values: Rang 1 to 30.
`static int` | `DEC_ES_FIXED_GAIN` If exposure mode is FIXED, what is the gain Valid Values: Rang 1 to 4.
`static int` | `DEC_ES_MAX_EXP` This is the maximum exposure allowed to use Valid Values: Rang 1 to 7874.
`static int` | `DEC_ES_MAX_GAIN` This is the maximum gain allowed to use Valid Values: Rang 1 to 4.
`static int` | `DEC_ES_TARGET_ACCEPT_GAP` How close to the target while value must image be Valid Values: Rang 1 to 50.
`static int` | `DEC_ES_TARGET_PERCENTILE` The percentile the white target value should be at Valid Values: Rang 1 to 99.
`static int` | `DEC_ES_TARGET_VALUE` Target white value in image to try and achieve Valid Values: Rang 1 to 255.
`static int` | `DEC_OCR_MODE` Note: The parameter values below are ONLY supported on platforms interfacing to the Honeywell 6703/6603 scanner.
`static int` | `DEC_OCR_TEMPLATE` Note: The parameter values below are ONLY supported on platforms interfacing to the Honeywell 6703/6603 scanner.
`static int` | `DEC_OCR_USER_TEMPLATE` Note: The parameter values below are ONLY supported on platforms interfacing to the Honeywell 6703/6603 scanner.
`static int` | `DEC_ILLUM_POWER_LEVEL` This parameter sets the level of illumination by altering laser/LED power. Power Level(1/2/3/4/5/6/7).
`static int` | `DEC_PICKLIST_AIM_DELAY` Note: The parameter values below are ONLY supported on platforms interfacing to the Honeywell 3680 scanner.
`static int` | `DEC_PICKLIST_AIM_MODE` Note: The parameter values below are ONLY supported on platforms interfacing to the Honeywell 3680 scanner.
`static int` | `DOTCODE_ENABLE` This property specifies whether Dotcode decoding is enabled.
`static int` | `DPM_DECODE_MODE` This property specifies whether DPM decoding is enabled during the execution of Decode.
`static int` | `EAN_EXT_ENABLE_2_5_DIGIT` This parameter determines whether or not EAN supplemental 2/5 should be transmitted.
`static int` | `EAN13_BOOKLAND_FORMAT` Select one of the following formats for Bookland data: 0 : Bookland ISBN-10; The decoder reports Bookland data starting with 978 in traditional 10-digit format with the special Bookland check digit for backward-compatibility.
`static int` | `EAN13_BOOKLANDEAN` This property specifies Enable or disable Bookland EAN.
`static int` | `EAN13_ENABLE` This property specifies whether EAN-13 decoding is enabled.
`static int` | `EAN13_SEND_CHECK` This property specifies whether transmit EAN-13 check digit.
`static int` | `EAN8_ENABLE` This property specifies whether EAN-8 decoding is enabled.
`static int` | `EAN8_SEND_CHECK` This property specifies whether transmit EAN-8 check digit.
`static int` | `EAN8_TO_EAN13` Enable this parameter to add five leading zeros to decoded EAN-8 symbols to make them compatible in format to EAN-13 symbols.
`static int` | `FULL_READ_MODE` Note: The property value below is ONLY supported on platforms interfacing to the Zebra Technologies imagers.
`static int` | `FUZZY_1D_PROCESSING` This option is enabled by default to optimize decode performance on 1D bar codes, including damaged and poor quality symbols.
`static int` | `GOOD_READ_BEEP_ENABLE` To set Scanner success beep when keystroke output enable `WEDGE_KEYBOARD_ENABLE`. Select valid value from the following options： 0 : None 1 : Short 2 : Sharp
`static int` | `GOOD_READ_VIBRATE_ENABLE` To set Scanner success vibrate when keystroke output enable.
`static int` | `GS1_14_ENABLE` This property specifies whether GS1 DataBar-14 decoding is enabled.
`static int` | `GS1_14_TO_UPC_EAN` This parameter only applies to GS1 DataBar-14 and GS1 DataBar Limited symbols not decoded as part of a Composite symbol.
`static int` | `GS1_EXP_ENABLE` This property specifies whether GS1 DataBar Expanded decoding is enabled.
`static int` | `GS1_EXP_LENGTH1` Set minimun length for GS1 DataBar Expanded. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `GS1_EXP_LENGTH2` Set maximun length for GS1 DataBar Expanded. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `GS1_LIMIT_ENABLE` This property specifies whether GS1 DataBar Limited decoding is enabled.
`static int` | `GS1_LIMIT_Security_Level` There are four levels of decode security for GS1 DataBar Limited bar codes.
`static int` | `GS1128__UCCEAN_Composite` GS1-128 Emulation Mode for UCC/EAN Composite Codes.
`static int` | `HANXIN_ENABLE` This property specifies whether Han Xin decoding is enabled.
`static int` | `HANXIN_INVERSE` Note: The parameter values below are ONLY supported on platforms interfacing to the Zebra Technologies imagers.
`static int` | `I25_ENABLE` This property specifies whether Interleaved 2 of 5 decoding is enabled.
`static int` | `I25_ENABLE_CHECK` Enable this feature to check the integrity of all I 2 of 5 symbols to verify the data complies with either the specified Uniform Symbology Specification (USS), or the Optical Product Code Council (OPCC) check digit algorithm.
`static int` | `I25_LENGTH1` Set minimun length for Interleaved 2 of 5. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `I25_LENGTH2` Set maximun length for Interleaved 2 of 5. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `I25_QUIET_ZONE` Enable or disable decoding I 2 of 5 bar codes with reduced quiet zones The property value should be set as follows: 0: Disallow short quiet zone symbols.
`static int` | `I25_SECURITY_LEVEL` Interleaved 2 of 5 bar codes are vulnerable to misdecodes, particularly when I 2 of 5 Lengths is set to Any Length.
`static int` | `I25_SEND_CHECK` This property specifies whetherto transmit I 2 of 5 data with or without the check digit.
`static int` | `I25_TO_EAN13` Enable this parameter to convert 14-character I 2 of 5 codes to EAN-13, and transmit to the host as EAN-13.
`static int` | `IMAGE_EXPOSURE_MODE` This property specifies the exposure mode that will be used during image capture.
`static int` | `IMAGE_FIXED_EXPOSURE` If exposure mode is FIXED, what is the exposure `IMAGE_FIXED_EXPOSURE`.
`static int` | `IMAGE_ONE_D_INVERSE` This property specifies whether the 1D inverse decoder setting: 0 : Regular Only; the decoder decodes regular 1D bar codes only.
`static int` | `IMAGE_PICKLIST_MODE` To set 2D Scanner Mobile Phone/Display Mode. This mode improves bar code reading performance on mobile phones and electronic displays.
`static int` | `JAPANESE_POST_ENABLE` This property specifies whether Japan Postal decoding is enabled.
`static int` | `KIX_CODE_ENABLE` This property specifies whether Netherlands KIX Code decoding is enabled.
`static int` | `LABEL_APPEND_ENTER` To set Scanner success append the action key character when keystroke output enable. Select valid value from the following options： 0 : None 1 : Carriage return 2 : IME action done 3 : TAB
`static int` | `LABEL_FORMAT_SEPARATOR_CHAR` When a bar code is scanned, the bar code data contains the Group Seperator char will hava replace `LABEL_SEPARATOR_ENABLE`.
`static int` | `LABEL_MATCHER_PATTERN` When a bar code is scanned, changed the bar code data with this form of regular expression.
`static int` | `LABEL_MATCHER_REPLACEMENT` When a bar code is scanned, with the Hex value characters to replace the bar code data, if it is contains `LABEL_MATCHER_TARGETREGEX` setting hex characters.
`static int` | `LABEL_MATCHER_TARGETREGEX` When a bar code is scanned, the bar code data contains the Hex value characters will hava replace `LABEL_MATCHER_REPLACEMENT` set the replace source characters are Hex value characters.Example:this “j” Hex ID is “6A”.
`static int` | `LABEL_PREFIX` When a bar code is scanned, additional Prefix characters is sent to the App along with the bar code data.
`static int` | `LABEL_SEPARATOR_ENABLE` This property specifies whether the bar code data replace the separator char `LABEL_FORMAT_SEPARATOR_CHAR`.
`static int` | `LABEL_SUFFIX` When a bar code is scanned, additional Suffix characters is sent to the App along with the bar code data.
`static int` | `LASER_ON_TIME` Set the maximum time decode processing continues during a scan attempt.
`static int` | `LINEAR_1D_QUIET_ZONE_LEVEL` This feature sets the level of aggressiveness in decoding bar codes with a reduced quiet zone (the area in front of and at the end of a bar code), and applies to symbologies enabled by a Reduced Quiet Zone parameter.
`static int` | `LINEAR_CODE_TYPE_SECURITY_LEVEL` To set Scanner linear code type security level. Parameters Values:0 to 3, default 1.
`static int` | `M25_ENABLE` This property specifies whether Matrix 2 of 5 decoding is enabled.
`static int` | `M25_ENABLE_CHECK` The check digit is the last character of the symbol used to verify the integrity of the data.
`static int` | `M25_LENGTH1` Set minimun length for Matrix 2 of 5. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `M25_LENGTH2` Set maximun length for Matrix 2 of 5. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `M25_SEND_CHECK` This property specifies whether to transmit Matrix 2 of 5 data with or without the check digit.
`static int` | `MAXICODE_ENABLE` This property specifies whether MaxiCode decoding is enabled.
`static int` | `MICROPDF417_ENABLE` This property specifies whether MicroPDF417 decoding is enabled.
`static int` | `MICROQRCODE_ENABLE` This property specifies whether MicroQR Code decoding is enabled.
`static int` | `MSI_CHECK_2_MOD_11` Select one of two algorithms for the verification of the second MSI check digit: 1 : MOD 10/MOD 10 0 : MOD 10/MOD 11
`static int` | `MSI_ENABLE` This property specifies whether MSI decoding is enabled.
`static int` | `MSI_LENGTH1` Set minimun length for MSI. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `MSI_LENGTH2` Set maximun length for MSI. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
`static int` | `MSI_REQUIRE_2_CHECK` With MSI symbols, one check digit is mandatory and always verified by the reader.
`static int` | `MSI_SEND_CHECK` Select whether to transmit MSI data with or without the check digit.
`static int` | `PDF417_ENABLE` This property specifies whether PDF417 decoding is enabled.
`static int` | `QRCODE_ENABLE` This property specifies whether QR Code decoding is enabled.
`static int` | `QRCODE_INVERSE` Note: The parameter values below are ONLY supported on platforms interfacing to the Zebra Technologies imagers.
`static int` | `REMOVE_NONPRINT_CHAR` This property specifies whether the bar code data remove the nonprint char.
`static int` | `ROYAL_MAIL_ENABLE` This property specifies whether ROYAL mail decoding is enabled.
`static int` | `SEND_GOOD_READ_BEEP_ENABLE` To set Scanner success beep or vibrate when SendBroadcast. SendBroadcast Values: `WEDGE_INTENT_ACTION_NAME` and `WEDGE_INTENT_DATA_STRING_TAG`.
`static int` | `SEND_GOOD_READ_VIBRATE_ENABLE` To set Scanner success vibrate when SendBroadcast. SendBroadcast Values: `WEDGE_INTENT_ACTION_NAME` and `WEDGE_INTENT_DATA_STRING_TAG`.
`static int` | `SEND_LABEL_PREFIX_SUFFIX` This property specifies whether Data format mode.
`static int` | `TIMEOUT_BETWEEN_SAME_SYMBOL` To set Scanner decoding timeout between same symbol. Parameters Values: value * 100 ms; value is 1 to 99, default 10.
`static int` | `TRANSMIT_CODE_ID` A Code ID character identifies the code type of a scanned bar code.
`static int` | `TRIGGERING_LOCK` This property specifies whether the scan trigger inactive (disable the scan button).
`static int` | `TRIGGERING_MODES` To set Scanner trigger modes. Parameters Values: `Triggering`
`static int` | `TRIOPTIC_ENABLE` This property specifies whether Trioptic decoding is enabled.
`static int` | `UCC_COUPON_EXT_CODE` Enable this parameter to decode UPC-A bar codes starting with digit ‘5’, EAN-13 bar codes starting with digit ‘99’, and UPC-A/EAN-128 Coupon Codes.
`static int` | `UCC_COUPON_EXT_REPORT_MODE` Traditional coupon symbols (old coupon symbols) are composed of two bar codes: UPC/EAN and Code128.
`static int` | `UCC_EAN_ZERO_EXTEND` Enable this parameter to add five leading zeros to decoded EAN-8 symbols to make them compatible in format to EAN-13 symbols.
`static int` | `UCC_REDUCED_QUIET_ZONE` Enable or disable decoding UPC bar codes with reduced quiet zones.
`static int` | `UPC_EAN_SECURITY_LEVEL` To set Scanner linear code type security level. Parameters Values: 0 to 3, default 1.
`static int` | `UPCA_ENABLE` This property specifies whether UPC-A decoding is enabled.
`static int` | `UPCA_SEND_CHECK` The check digit is the last character of the symbol used to verify the integrity of the data.
`static int` | `UPCA_SEND_SYS` Preamble characters are part of the UPC symbol, and include Country Code and System Character.
`static int` | `UPCA_TO_EAN13` When UPC-A Converted to EAN-13 is selected, UPC-A bar codes are converted to 13 digit EAN-13 codes by adding a zero to the front.
`static int` | `UPCE_ENABLE` This property specifies whether UPC-E decoding is enabled.
`static int` | `UPCE_SEND_CHECK` The check digit is the last character of the symbol used to verify the integrity of the data.
`static int` | `UPCE_SEND_SYS` Preamble characters are part of the UPC symbol, and include Country Code and System Character.
`static int` | `UPCE_TO_UPCA` Enable this to convert UPC-E (zero suppressed) decoded data to UPC-A format before transmission.
`static int` | `UPCE1_ENABLE` This property specifies whether UPC-E1 decoding is enabled.
`static int` | `UPCE1_SEND_CHECK` The check digit is the last character of the symbol used to verify the integrity of the data.
`static int` | `UPCE1_SEND_SYS` Preamble characters are part of the UPC symbol, and include Country Code and System Character.
`static int` | `UPCE1_TO_UPCA` Enable this to convert UPC-E1 decoded data to UPC-A format before transmission.
`static int` | `UPU_FICS_ENABLE` This property specifies whether UPU FICS Postal decoding is enabled.
`static int` | `US_PLANET_ENABLE` This property specifies whether US Planet decoding is enabled.
`static int` | `US_POSTAL_SEND_CHECK` Select whether to transmit US Postal data, which includes both US Postnet and US Planet, with or without the check digit.
`static int` | `US_POSTNET_ENABLE` This property specifies whether US Postnet/US Postal decoding is enabled.
`static int` | `USPS_4STATE_ENABLE` This property specifies whether USPS 4CB/One Code/Intelligent Mail decoding is enabled.
`static int` | `WEDGE_INTENT_ACTION_NAME` The intent action name is to receive barcode data. The default is "android.intent.ACTION_DECODE_DATA".
`static int` | `WEDGE_INTENT_DATA_STRING_TAG` A string tag represents the barcode string. The default is "barcode_string".
`static int` | `WEDGE_INTENT_LABEL_TYPE_TAG` A string tag represents the barcode type. The default is "barcodeType".
`static int` | `WEDGE_KEYBOARD_ENABLE` This property specifies whether Keyboard mode is enabled. If the configured PropertyID.WEDGE_KEYBOARD_ENABLE is 1, append the barcode text to TextBox, input method, or send the barcode text as key events.
`static int` | `WEDGE_KEYBOARD_TYPE` This property specifies select an option for keystroke types. Values: 0 : Auto append text to TextBox. 1 : If there is no TextBox, append text to input method. 2 : Send key event. 3 : Auto append text to input method.

Constructor Summary
`PropertyID()` PropertyID class contains all supported Scanner sub-system reader properties.

Method Summary

Methods inherited from class java.lang.Object
`equals, getClass, hashCode, notify, notifyAll, toString, wait, wait, wait`

FIELD DETAIL

### SEND_GOOD_READ_BEEP_ENABLE

    public static final int SEND_GOOD_READ_BEEP_ENABLE

  To set Scanner success beep or vibrate when SendBroadcast. SendBroadcast Values:
  `WEDGE_INTENT_ACTION_NAME` and `WEDGE_INTENT_DATA_STRING_TAG`.

  See Also:
    Constant Field Values

### SEND_GOOD_READ_VIBRATE_ENABLE

    public static final int SEND_GOOD_READ_VIBRATE_ENABLE

  To set Scanner success vibrate when SendBroadcast. SendBroadcast Values:
  `WEDGE_INTENT_ACTION_NAME` and `WEDGE_INTENT_DATA_STRING_TAG`.
  See Also:
    Constant Field Values

### TRIGGERING_MODES

    public static final int TRIGGERING_MODES

  To set Scanner trigger modes Parameters Values: `Triggering`

  See Also:
    Constant Field Values

### GOOD_READ_BEEP_ENABLE

    public static final int GOOD_READ_BEEP_ENABLE

  To set Scanner success beep when keystroke output enable `WEDGE_KEYBOARD_ENABLE`. Select valid value from the following options： 0 : None 1 : Short 2 : Sharp
  See Also:
    Constant Field Values

### GOOD_READ_VIBRATE_ENABLE

    public static final int GOOD_READ_VIBRATE_ENABLE

  To set Scanner success vibrate when keystroke output enable.
  See Also:
    Constant Field Values

### LABEL_APPEND_ENTER

    public static final int LABEL_APPEND_ENTER

  To set Scanner success append the action key character when keystroke output enable. Select valid value from the following options： 0 : None 1 : Carriage return 2 : IME action done 3 : TAB
  See Also:
    Constant Field Values

### LABEL_FORMAT_SEPARATOR_CHAR

    public static final int LABEL_FORMAT_SEPARATOR_CHAR

  When a bar code is scanned, the bar code data contains the Group Seperator char will hava replace `LABEL_SEPARATOR_ENABLE`.
  See Also:
    Constant Field Values

### IMAGE_PICKLIST_MODE

    public static final int IMAGE_PICKLIST_MODE

  To set 2D Scanner Mobile Phone/Display Mode.This mode improves bar code reading performance on mobile phones and electronic displays.

  See Also:
    Constant Field Values

### TRANSMIT_CODE_ID

    public static final int TRANSMIT_CODE_ID

  A Code ID character identifies the code type of a scanned bar code.
  See Also:
    Constant Field Values

### TRIGGERING_LOCK

    public static final int TRIGGERING_LOCK

  This property specifies whether the scan trigger inactive (disable the scan button).
  See Also:
    Constant Field Values

### IMAGE_ONE_D_INVERSE

    public static final int IMAGE_ONE_D_INVERSE

  This property specifies whether the 1D inverse decoder setting: 0 : Regular Only; the decoder decodes regular 1D bar codes only.

  See Also:
    Constant Field Values

### LABEL_MATCHER_PATTERN

    public static final int LABEL_MATCHER_PATTERN

  When a bar code is scanned, changed the bar code data with this form of regular expression.
  See Also:
    Constant Field Values

### LABEL_MATCHER_REPLACEMENT

    public static final int LABEL_MATCHER_REPLACEMENT

  When a bar code is scanned, with the Hex value characters to replace the bar code data, if it is contains `LABEL_MATCHER_TARGETREGEX` setting hex characters.
  See Also:
    Constant Field Values

### LABEL_MATCHER_TARGETREGEX

    public static final int LABEL_MATCHER_TARGETREGEX

  When a bar code is scanned, the bar code data contains the Hex value characters will hava replace `LABEL_MATCHER_REPLACEMENT` set the replace source characters are Hex value characters.Example:this “j” Hex ID is “6A”.
  See Also:
    Constant Field Values

### SEND_LABEL_PREFIX_SUFFIX

    public static final int SEND_LABEL_PREFIX_SUFFIX

  This property specifies whether Data format mode.
  See Also:
    Constant Field Values

### LABEL_PREFIX

    public static final int LABEL_PREFIX

  When a bar code is scanned, additional Prefix characters is sent to the App along with the bar code data.
  See Also:
    Constant Field Values

### LABEL_SEPARATOR_ENABLE

    public static final int LABEL_SEPARATOR_ENABLE

  This property specifies whether the bar code data replace the separator char `LABEL_FORMAT_SEPARATOR_CHAR`.
  See Also:
    Constant Field Values

### LABEL_SUFFIX

    public static final int LABEL_SUFFIX

  When a bar code is scanned, additional Suffix characters is sent to the App along with the bar code data.
  See Also:
    Constant Field Values

### LASER_ON_TIME

    public static final int LASER_ON_TIME

  Set the maximum time decode processing continues during a scan attempt.

  See Also:
    Constant Field Values

### TIMEOUT_BETWEEN_SAME_SYMBOL

    public static final int TIMEOUT_BETWEEN_SAME_SYMBOL

  To set Scanner decoding timeout between same symbol. Parameters Values: value * 100 ms; value is 1 to 99, default 10.

  See Also:
    Constant Field Values

### LINEAR_1D_QUIET_ZONE_LEVEL

    public static final int LINEAR_1D_QUIET_ZONE_LEVEL

  This feature sets the level of aggressiveness in decoding bar codes with a reduced quiet zone (the area in front of and at the end of a bar code), and applies to symbologies enabled by a Reduced Quiet Zone parameter.

  See Also:
    Constant Field Values

### LINEAR_CODE_TYPE_SECURITY_LEVEL

    public static final int LINEAR_CODE_TYPE_SECURITY_LEVEL

  To set Scanner linear code type security level. Parameters Values:0 to 3, default 1.

  See Also:
    Constant Field Values

### FULL_READ_MODE

    public static final int FULL_READ_MODE

  Note: The property value below is ONLY supported on platforms interfacing to the Zebra Technologies imagers.
  See Also:
    Constant Field Values

### FUZZY_1D_PROCESSING

    public static final int FUZZY_1D_PROCESSING

  This option is enabled by default to optimize decode performance on 1D bar codes, including damaged and poor quality symbols.
  See Also:
    Constant Field Values

### CODING_FORMAT

    public static final int CODING_FORMAT

  This property specifies the character encoding to use for the bar code data.
  See Also:
    Constant Field Values

### IMAGE_EXPOSURE_MODE

    public static final int IMAGE_EXPOSURE_MODE

  This property specifies the exposure mode that will be used during image capture.
  See Also:
    Constant Field Values

### IMAGE_FIXED_EXPOSURE

    public static final int IMAGE_FIXED_EXPOSURE

  If exposure mode is FIXED, what is the exposure `IMAGE_FIXED_EXPOSURE`.
  See Also:
    Constant Field Values

### CODE39_ENABLE

    public static final int CODE39_ENABLE

  This property specifies whether Code39 decoding is enabled.
  See Also:
    Constant Field Values

### CODE39_ENABLE_CHECK

    public static final int CODE39_ENABLE_CHECK

  Enable this to check the integrity of all Code39 symbols to verify that the data complies with specified check digit algorithm.
  See Also:
    Constant Field Values

### CODE39_SEND_CHECK

    public static final int CODE39_SEND_CHECK

  This property specifies whether to transmit Code39 data with or without the check digit.
  See Also:
    Constant Field Values

### CODE39_START_STOP

    public static final int CODE39_START_STOP

  Start/Stop characters identify the leading and trailing ends of the bar code.
  See Also:
    Constant Field Values

### CODE39_FULL_ASCII

    public static final int CODE39_FULL_ASCII

  Code39 Full ASCII is a variant of Code39 which pairs characters to encode the full ASCII character set.
  See Also:
    Constant Field Values

### CODE39_LENGTH1

    public static final int CODE39_LENGTH1

  Set minimun length for Code39. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### CODE39_LENGTH2

    public static final int CODE39_LENGTH2

  Set maximun length for Code39. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### CODE39_Quiet_Zone

    public static final int CODE39_Quiet_Zone

  Enable or disable decoding Code39 bar codes with reduced quiet zones.
  See Also:
    Constant Field Values

### CODE39_SECURITY_LEVEL

    public static final int CODE39_SECURITY_LEVEL

  The scanner offers four levels of decode security for Code39 barcodes.
  See Also:
    Constant Field Values

### TRIOPTIC_ENABLE

    public static final int TRIOPTIC_ENABLE

  This property specifies whether Trioptic decoding is enabled.
  See Also:
    Constant Field Values

### CODE32_ENABLE

    public static final int CODE32_ENABLE

  This property specifies whether Code32 decoding is enabled.
  See Also:
    Constant Field Values

### CODE32_SEND_START

    public static final int CODE32_SEND_START

  Enable or disable adding the prefix character “A” to all Code32 bar codes.
  See Also:
    Constant Field Values

### C25_ENABLE

    public static final int C25_ENABLE

  This property specifies whether chinese 2 of 5 post decoding is enabled.
  See Also:
    Constant Field Values

### D25_ENABLE

    public static final int D25_ENABLE

  This property specifies whether Discrete 2 of 5 decoding is enabled.
  See Also:
    Constant Field Values

### D25_LENGTH1

    public static final int D25_LENGTH1

  Set minimun length for Discrete 2 of 5. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### D25_LENGTH2

    public static final int D25_LENGTH2

  Set maximun length for Discrete 2 of 5. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### M25_ENABLE

    public static final int M25_ENABLE

  This property specifies whether Matrix 2 of 5 decoding is enabled.
  See Also:
    Constant Field Values

### M25_ENABLE_CHECK

    public static final int M25_ENABLE_CHECK

  The check digit is the last character of the symbol used to verify the integrity of the data.
  See Also:
    Constant Field Values

### M25_LENGTH1

    public static final int M25_LENGTH1

  Set minimun length for Matrix 2 of 5. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### M25_LENGTH2

    public static final int M25_LENGTH2

  Set maximun length for Matrix 2 of 5. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### M25_SEND_CHECK

    public static final int M25_SEND_CHECK

  This property specifies whether to transmit Matrix 2 of 5 data with or without the check digit.
  See Also:
    Constant Field Values

### CODE11_ENABLE

    public static final int CODE11_ENABLE

  This property specifies whether Code11 decoding is enabled.
  See Also:
    Constant Field Values

### CODE11_ENABLE_CHECK

    public static final int CODE11_ENABLE_CHECK

  This feature allows the decoder to check the integrity of all Code11 symbols to verify that the data complies with the specified check digit algorithm.
  See Also:
    Constant Field Values

### CODE11_SEND_CHECK

    public static final int CODE11_SEND_CHECK

  This property specifies whether or not to transmit the Code11 check digit(s).
  See Also:
    Constant Field Values

### CODE128_CHECK_ISBT_TABLE

    public static final int CODE128_CHECK_ISBT_TABLE

  The ISBT specification includes a table that lists several types of ISBT bar codes that are commonly used in pairs.
  See Also:
    Constant Field Values

### CODE11_LENGTH1

    public static final int CODE11_LENGTH1

  Set minimun length for Code11. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### CODE11_LENGTH2

    public static final int CODE11_LENGTH2

  Set maximun length for Code11. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### I25_ENABLE

    public static final int I25_ENABLE

  This property specifies whether Interleaved 2 of 5 decoding is enabled.
  See Also:
    Constant Field Values

### I25_ENABLE_CHECK

    public static final int I25_ENABLE_CHECK

  Enable this feature to check the integrity of all I 2 of 5 symbols to verify the data complies with either the specified Uniform Symbology Specification (USS), or the Optical Product Code Council (OPCC) check digit algorithm.
  See Also:
    Constant Field Values

### I25_SEND_CHECK

    public static final int I25_SEND_CHECK

  This property specifies whetherto transmit I 2 of 5 data with or without the check digit.
  See Also:
    Constant Field Values

### I25_LENGTH1

    public static final int I25_LENGTH1

  Set minimun length for Interleaved 2 of 5. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### I25_LENGTH2

    public static final int I25_LENGTH2

  Set maximun length for Interleaved 2 of 5. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### I25_QUIET_ZONE

    public static final int I25_QUIET_ZONE

  Enable or disable decoding I 2 of 5 bar codes with reduced quiet zones The property value should be set as follows: 0: Disallow short quiet zone symbols.
  See Also:
    Constant Field Values

### I25_SECURITY_LEVEL

    public static final int I25_SECURITY_LEVEL

  Interleaved 2 of 5 bar codes are vulnerable to misdecodes, particularly when I 2 of 5 Lengths is set to Any Length.
  See Also:
    Constant Field Values

### I25_TO_EAN13

    public static final int I25_TO_EAN13

  Enable this parameter to convert 14-character I 2 of 5 codes to EAN-13, and transmit to the host as EAN-13.
  See Also:
    Constant Field Values

### CODABAR_ENABLE

    public static final int CODABAR_ENABLE

  This property specifies whether Codabar decoding is enabled.
  See Also:
    Constant Field Values

### CODABAR_ENABLE_CHECK

    public static final int CODABAR_ENABLE_CHECK

  This property specifies whether Codabar check digit verification is enable.
  See Also:
    Constant Field Values

### CODABAR_NOTIS

    public static final int CODABAR_NOTIS

  Enable this parameter to strip the start and stop characters from a decoded Codabar symbol.
  See Also:
    Constant Field Values

### CODABAR_SEND_CHECK

    public static final int CODABAR_SEND_CHECK

  This property specifies whetherto transmit Codabar data with or without the check digit.
  See Also:
    Constant Field Values

### CODABAR_SEND_START

    public static final int CODABAR_SEND_START

  Start/Stop characters identify the leading and trailing ends of the bar code.
  See Also:
    Constant Field Values

### CODABAR_CLSI

    public static final int CODABAR_CLSI

  Enable this parameter to strip the start and stop characters and insert a space after the first, fifth, and tenth characters of a 14-character Codabar symbol.
  See Also:
    Constant Field Values

### CODABAR_LENGTH1

    public static final int CODABAR_LENGTH1

  Set minimun length for Codabar. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### CODABAR_LENGTH2

    public static final int CODABAR_LENGTH2

  Set maximun length for Codabar. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### CODE93_ENABLE

    public static final int CODE93_ENABLE

  This property specifies whether Code93 decoding is enabled.
  See Also:
    Constant Field Values

### CODE93_LENGTH1

    public static final int CODE93_LENGTH1

  Set minimun length for Code39. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### CODE93_LENGTH2

    public static final int CODE93_LENGTH2

  Set maximun length for Code39. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### CODE128_ENABLE

    public static final int CODE128_ENABLE

  This property specifies whether Code128 decoding is enabled.
  See Also:
    Constant Field Values

### CODE128_LENGTH1

    public static final int CODE128_LENGTH1

  Set minimun length for Code128. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### CODE128_LENGTH2

    public static final int CODE128_LENGTH2

  Set maximun length for Code128. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### CODE128_REDUCED_QUIET_ZONE

    public static final int CODE128_REDUCED_QUIET_ZONE

  Enable or disable decoding Code128 bar codes with reduced quiet zones. The property value should be set as follows: 0 : Disallow short quiet zone symbols.
  See Also:
    Constant Field Values

### CODE128_SECURITY_LEVEL

    public static final int CODE128_SECURITY_LEVEL

  Code128 bar codes are vulnerable to misdecodes, particularly when Code128 Lengths is set to Any Length.
  See Also:
    Constant Field Values

### CODE_ISBT_128

    public static final int CODE_ISBT_128

  ISBT 128 is a variant of Code128 used in the blood bank industry.
  See Also:
    Constant Field Values

### CODE_ISBT_Concatenation_MODE

    public static final int CODE_ISBT_Concatenation_MODE

  Select an option for concatenating pairs of ISBT code types:
  0 : Disable ISBT Concatenation - The device does not concatenate pairs of ISBT codes it encounters.
  See Also:
    Constant Field Values

### CODE128_GS1_ENABLE

    public static final int CODE128_GS1_ENABLE

  This property specifies whether GS1-128 decoding is enabled.
  See Also:
    Constant Field Values

### CODE128_IGNORE_FNC4

    public static final int CODE128_IGNORE_FNC4

  This feature applies to Code128 bar codes with an embedded character.
  0 : Disable Ignore Code128; The character is not transmitted but the following character has 128 added to it.
  1 : Enable Ignore Code128; This strips the character from the decode data. The remaining characters do not change.
  See Also:
    Constant Field Values

### UPCA_ENABLE

    public static final int UPCA_ENABLE

  This property specifies whether UPC-A decoding is enabled.
  See Also:
    Constant Field Values

### UPCA_SEND_CHECK

    public static final int UPCA_SEND_CHECK

  The check digit is the last character of the symbol used to verify the integrity of the data.
  See Also:
    Constant Field Values

### UPCA_SEND_SYS

    public static final int UPCA_SEND_SYS

  Preamble characters are part of the UPC symbol, and include Country Code and System Character.
  See Also:
    Constant Field Values

### UPCA_TO_EAN13

    public static final int UPCA_TO_EAN13

  When UPC-A Converted to EAN-13 is selected, UPC-A bar codes are converted to 13 digit EAN-13 codes by adding a zero to the front.
  See Also:
    Constant Field Values

### UPCE_ENABLE

    public static final int UPCE_ENABLE

  This property specifies whether UPC-E decoding is enabled.
  See Also:
    Constant Field Values

### UPCE_SEND_CHECK

    public static final int UPCE_SEND_CHECK

  The check digit is the last character of the symbol used to verify the integrity of the data.
  See Also:
    Constant Field Values

### UPCE_SEND_SYS

    public static final int UPCE_SEND_SYS

  Preamble characters are part of the UPC symbol, and include Country Code and System Character.
  See Also:
    Constant Field Values

### UPCE_TO_UPCA

    public static final int UPCE_TO_UPCA

  Enable this to convert UPC-E (zero suppressed) decoded data to UPC-A format before transmission.
  See Also:
    Constant Field Values

### UPCE1_ENABLE

    public static final int UPCE1_ENABLE

  This property specifies whether UPC-E1 decoding is enabled.
  See Also:
    Constant Field Values

### UPCE1_SEND_CHECK

    public static final int UPCE1_SEND_CHECK

  The check digit is the last character of the symbol used to verify the integrity of the data.
  See Also:
    Constant Field Values

### UPCE1_SEND_SYS

    public static final int UPCE1_SEND_SYS

  Preamble characters are part of the UPC symbol, and include Country Code and System Character.
  See Also:
    Constant Field Values

### UPCE1_TO_UPCA

    public static final int UPCE1_TO_UPCA

  Enable this to convert UPC-E1 decoded data to UPC-A format before transmission.
  See Also:
    Constant Field Values

### EAN13_ENABLE

    public static final int EAN13_ENABLE

  This property specifies whether EAN-13 decoding is enabled.
  See Also:
    Constant Field Values

### EAN13_SEND_CHECK

    public static final int EAN13_SEND_CHECK

  This property specifies whether transmit EAN-13 check digit.
  See Also:
    Constant Field Values

### EAN13_BOOKLANDEAN

    public static final int EAN13_BOOKLANDEAN

  This property specifies Enable or disable Bookland EAN.
  See Also:
    Constant Field Values

### EAN13_BOOKLAND_FORMAT

    public static final int EAN13_BOOKLAND_FORMAT

  Select one of the following formats for Bookland data: 0 : Bookland ISBN-10; The decoder reports Bookland data starting with 978 in traditional 10-digit format with the special Bookland check digit for backward-compatibility.
  See Also:
    Constant Field Values

### EAN8_ENABLE

    public static final int EAN8_ENABLE

  This property specifies whether EAN-8 decoding is enabled.
  See Also:
    Constant Field Values

### EAN8_SEND_CHECK

    public static final int EAN8_SEND_CHECK

  This property specifies whether transmit EAN-8 check digit.
  See Also:
    Constant Field Values

### EAN8_TO_EAN13

    public static final int EAN8_TO_EAN13

  Enable this parameter to add five leading zeros to decoded EAN-8 symbols to make them compatible in format to EAN-13 symbols.
  See Also:
    Constant Field Values

### EAN_EXT_ENABLE_2_5_DIGIT

    public static final int EAN_EXT_ENABLE_2_5_DIGIT

  This parameter determines whether or not EAN supplemental 2/5 should be transmitted.
  See Also:
    Constant Field Values

### UPC_EAN_SECURITY_LEVEL

    public static final int UPC_EAN_SECURITY_LEVEL

  To set Scanner linear code type security level. Parameters Values: 0 to 3, default 1.

  See Also:
    Constant Field Values

### UCC_COUPON_EXT_CODE

    public static final int UCC_COUPON_EXT_CODE

  Traditional coupon symbols (old coupon symbols) are composed of two bar codes: UPC/EAN and Code128.
  See Also:
    Constant Field Values

### UCC_COUPON_EXT_REPORT_MODE

    public static final int UCC_COUPON_EXT_REPORT_MODE

  Enable this parameter to add five leading zeros to decoded EAN-8 symbols to make them compatible in format to EAN-13 symbols.
  See Also:
    Constant Field Values

### UCC_EAN_ZERO_EXTEND

    public static final int UCC_EAN_ZERO_EXTEND

  Enable or disable decoding UPC bar codes with reduced quiet zones.
  See Also:
    Constant Field Values

### UCC_REDUCED_QUIET_ZONE

    public static final int UCC_REDUCED_QUIET_ZONE

  Enable this parameter to decode UPC-A bar codes starting with digit ‘5’, EAN-13 bar codes starting with digit ‘99’, and UPC-A/EAN-128 Coupon Codes.
  See Also:
    Constant Field Values

### MSI_ENABLE

    public static final int MSI_ENABLE

  This property specifies whether MSI decoding is enabled.
  See Also:
    Constant Field Values

### MSI_REQUIRE_2_CHECK

    public static final int MSI_REQUIRE_2_CHECK

  With MSI symbols, one check digit is mandatory and always verified by the reader.
  See Also:
    Constant Field Values

### MSI_SEND_CHECK

    public static final int MSI_SEND_CHECK

  Select whether to transmit MSI data with or without the check digit.
  See Also:
    Constant Field Values

### MSI_CHECK_2_MOD_11

    public static final int MSI_CHECK_2_MOD_11

  Select one of two algorithms for the verification of the second MSI check digit:
  1 : MOD 10/MOD 10
  0 : MOD 10/MOD 11
  See Also:
    Constant Field Values

### MSI_LENGTH1

    public static final int MSI_LENGTH1

  Set minimun length for MSI. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### MSI_LENGTH2

    public static final int MSI_LENGTH2

  Set maximun length for MSI. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### GS1_14_ENABLE

    public static final int GS1_14_ENABLE

  This property specifies whether GS1 DataBar-14 decoding is enabled.
  See Also:
    Constant Field Values

### GS1_14_TO_UPC_EAN

    public static final int GS1_14_TO_UPC_EAN

  This parameter only applies to GS1 DataBar-14 and GS1 DataBar Limited symbols not decoded as part of a Composite symbol.
  See Also:
    Constant Field Values

### GS1_LIMIT_ENABLE

    public static final int GS1_LIMIT_ENABLE

  This property specifies whether GS1 DataBar Limited decoding is enabled.
  See Also:
    Constant Field Values

### GS1_LIMIT_Security_Level

    public static final int GS1_LIMIT_Security_Level

  There are four levels of decode security for GS1 DataBar Limited bar codes.
  See Also:
    Constant Field Values

### GS1128__UCCEAN_Composite

    public static final int GS1128__UCCEAN_Composite

  GS1-128 Emulation Mode for UCC/EAN Composite Codes.
  See Also:
    Constant Field Values

### GS1_EXP_ENABLE

    public static final int GS1_EXP_ENABLE

  This property specifies whether GS1 DataBar Expanded decoding is enabled.
  See Also:
    Constant Field Values

### GS1_EXP_LENGTH1

    public static final int GS1_EXP_LENGTH1

  Set minimun length for GS1 DataBar Expanded. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### GS1_EXP_LENGTH2

    public static final int GS1_EXP_LENGTH2

  Set maximun length for GS1 DataBar Expanded. Range: 0 to 55. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### US_POSTNET_ENABLE

    public static final int US_POSTNET_ENABLE

  This property specifies whether US Postnet/US Postal decoding is enabled.
  See Also:
    Constant Field Values

### US_PLANET_ENABLE

    public static final int US_PLANET_ENABLE

  This property specifies whether US Planet decoding is enabled.
  See Also:
    Constant Field Values

### US_POSTAL_SEND_CHECK

    public static final int US_POSTAL_SEND_CHECK

  Select whether to transmit US Postal data, which includes both US Postnet and US Planet, with or without the check digit.
  See Also:
    Constant Field Values

### USPS_4STATE_ENABLE

    public static final int USPS_4STATE_ENABLE

  This property specifies whether USPS 4CB/One Code/Intelligent Mail decoding is enabled.
  See Also:
    Constant Field Values

### UPU_FICS_ENABLE

    public static final int UPU_FICS_ENABLE

  This property specifies whether UPU FICS Postal decoding is enabled.
  See Also:
    Constant Field Values

### ROYAL_MAIL_ENABLE

    public static final int ROYAL_MAIL_ENABLE

  This property specifies whether ROYAL mail decoding is enabled.
  See Also:
    Constant Field Values

### AUSTRALIAN_POST_ENABLE

    public static final int AUSTRALIAN_POST_ENABLE

  This property specifies whether Australia Post decoding is enabled.
  See Also:
    Constant Field Values

### KIX_CODE_ENABLE

    public static final int KIX_CODE_ENABLE

  This property specifies whether Netherlands KIX Code decoding is enabled.
  See Also:
    Constant Field Values

### JAPANESE_POST_ENABLE

    public static final int JAPANESE_POST_ENABLE

  This property specifies whether Japan Postal decoding is enabled.
  See Also:
    Constant Field Values

### PDF417_ENABLE

    public static final int PDF417_ENABLE

  This property specifies whether PDF417 decoding is enabled.
  See Also:
    Constant Field Values

### MICROPDF417_ENABLE

    public static final int MICROPDF417_ENABLE

  This property specifies whether MicroPDF417 decoding is enabled.
  See Also:
    Constant Field Values

### COMPOSITE_CC_AB_ENABLE

    public static final int COMPOSITE_CC_AB_ENABLE

  This property specifies whether Composite CC-A/B decoding is enabled.
  See Also:
    Constant Field Values

### COMPOSITE_CC_C_ENABLE

    public static final int COMPOSITE_CC_C_ENABLE

  This property specifies whether Composite CC-C decoding is enabled.
  See Also:
    Constant Field Values

### COMPOSITE_TLC39_ENABLE

    public static final int COMPOSITE_TLC39_ENABLE

  This property specifies whether Composite TLC-39 decoding is enabled.
  See Also:
    Constant Field Values

### HANXIN_ENABLE

    public static final int HANXIN_ENABLE

  This property specifies whether Han Xin decoding is enabled.
  See Also:
    Constant Field Values

### HANXIN_INVERSE

    public static final int HANXIN_INVERSE

  Note: The parameter values below are ONLY supported on platforms interfacing to the Zebra Technologies imagers.
  See Also:
    Constant Field Values

### DATAMATRIX_ENABLE

    public static final int DATAMATRIX_ENABLE

  This property specifies whether DataMatrix decoding is enabled.
  See Also:
    Constant Field Values

### DATAMATRIX_LENGTH1

    public static final int DATAMATRIX_LENGTH1

  Set minimun length for DataMatrix. Range: 1 to 3166. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### DATAMATRIX_LENGTH2

    public static final int DATAMATRIX_LENGTH2

  Set minimun length for DataMatrix. Range: 1 to 3166. The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  See Also:
    Constant Field Values

### DATAMATRIX_INVERSE

    public static final int DATAMATRIX_INVERSE

  Set the DATAMATRIX inverse decoder setting: Regular Only/ Inverse Only/ Inverse Autodetect. Note: The parameter values below are only supported on platforms interfacing to the Zebra Technologies imagers.
  See Also:
    Constant Field Values

### MAXICODE_ENABLE

    public static final int MAXICODE_ENABLE

  This property specifies whether MaxiCode decoding is enabled.
  See Also:
    Constant Field Values

### QRCODE_ENABLE

    public static final int QRCODE_ENABLE

  This property specifies whether QR Code decoding is enabled.
  See Also:
    Constant Field Values

### MICROQRCODE_ENABLE

    public static final int MICROQRCODE_ENABLE

  This property specifies whether MicroQR Code decoding is enabled.
  See Also:
    Constant Field Values

### QRCODE_INVERSE

    public static final int QRCODE_INVERSE

  Note: The parameter values below are ONLY supported on platforms interfacing to the Zebra Technologies imagers.
  See Also:
    Constant Field Values

### REMOVE_NONPRINT_CHAR

    public static final int REMOVE_NONPRINT_CHAR

  This property specifies whether the bar code data remove the nonprint char.
  See Also:
    Constant Field Values

### AZTEC_ENABLE

    public static final int AZTEC_ENABLE

  This property specifies whether Aztec Code decoding is enabled.
  See Also:
    Constant Field Values

### AZTEC_INVERSE

    public static final int AZTEC_INVERSE

  Set the Aztec inverse decoder setting: Regular Only/ Inverse Only/ Inverse Autodetect. Note: The parameter values below are ONLY supported on platforms interfacing to the Zebra Technologies imagers.
  See Also:
    Constant Field Values

### DEC_2D_LIGHTS_MODE

    public static final int DEC_2D_LIGHTS_MODE

  This property specifies whether the lights mode settings. Lights Configuration settings:(Illum/Aimer Off)/(Aimer Only)/(Illum Only)/(Alternating)/(Concurrent).
  See Also:
    Constant Field Values

### DEC_2D_CENTERING_ENABLE

    public static final int DEC_2D_CENTERING_ENABLE

  This property specifies whether Centering mode decoding is enabled.
  See Also:
    Constant Field Values

### DEC_2D_CENTERING_MODE

    public static final int DEC_2D_CENTERING_MODE

  Mode Configuration settings:Off/Around Aimer/Field Of View. Note: The parameter values below are ONLY supported on platforms interfacing to the Honeywell 6703/6603 scanner.
  See Also:
    Constant Field Values

### DEC_2D_WINDOW_UPPER_LX

    public static final int DEC_2D_WINDOW_UPPER_LX

  Upper left X coordinate setting : default 290, min 0, max 319.
  See Also:
    Constant Field Values

### DEC_2D_WINDOW_UPPER_LY

    public static final int DEC_2D_WINDOW_UPPER_LY

  Upper left Y coordinate setting :default 350, min 320, max 639.
  See Also:
    Constant Field Values

### DEC_ES_CONFORM_IMAGE

    public static final int DEC_ES_CONFORM_IMAGE

  The image must conform to the auto-exposure requirements, if not, it's rejected. Valid Values: Rang 0to 1.
  See Also:
    Constant Field Values

### DEC_ES_CONFORM_TRIES

    public static final int DEC_ES_CONFORM_TRIES

  The number of time it will attempt to conform Valid Values: Rang 1 to 8.
  See Also:
    Constant Field Values

### DEC_ES_FIXED_FRAME_RATE

    public static final int DEC_ES_FIXED_FRAME_RATE

  If exposure mode is FIXED, what is the frame rate (fixed, has no effect) Valid Values: Rang 1 to 30.
  See Also:
    Constant Field Values

### DEC_ES_FIXED_GAIN

    public static final int DEC_ES_FIXED_GAIN

  If exposure mode is FIXED, what is the gain Valid Values: Rang 1 to 4.
  See Also:
    Constant Field Values

### DEC_ES_MAX_EXP

    public static final int DEC_ES_MAX_EXP

  This is the maximum exposure allowed to use Valid Values: Rang 1 to 7874.
  See Also:
    Constant Field Values

### DEC_ES_MAX_GAIN

    public static final int DEC_ES_MAX_GAIN

  This is the maximum gain allowed to use Valid Values: Rang 1 to 4.
  See Also:
    Constant Field Values

### DEC_ES_TARGET_ACCEPT_GAP

    public static final int DEC_ES_TARGET_ACCEPT_GAP

  How close to the target while value must image be Valid Values: Rang 1 to 50.
  See Also:
    Constant Field Values

### DEC_ES_TARGET_PERCENTILE

    public static final int DEC_ES_TARGET_PERCENTILE

  The percentile the white target value should be at Valid Values: Rang 1 to 99.
  See Also:
    Constant Field Values

### DEC_ES_TARGET_VALUE

    public static final int DEC_ES_TARGET_VALUE

  Target white value in image to try and achieve Valid Values: Rang 1 to 255.
  See Also:
    Constant Field Values

### DEC_2D_WINDOW_LOWER_RX

    public static final int DEC_2D_WINDOW_LOWER_RX

  Upper right X coordinate setting : default 386, min 0, max 415.
  See Also:
    Constant Field Values

### DEC_2D_WINDOW_LOWER_RY

    public static final int DEC_2D_WINDOW_LOWER_RY

  Upper right Y coordinate setting : default 446, min 416, max 831.
  See Also:
    Constant Field Values

### DEC_OCR_MODE

    public static final int DEC_OCR_MODE

  Note: The parameter values below are ONLY supported on platforms interfacing to the Honeywell 6703/6603 scanner.
  See Also:
    Constant Field Values

### DEC_OCR_TEMPLATE

    public static final int DEC_OCR_TEMPLATE

  Note: The parameter values below are ONLY supported on platforms interfacing to the Honeywell 6703/6603 scanner.
  See Also:
    Constant Field Values

### DEC_OCR_USER_TEMPLATE

    public static final int DEC_OCR_USER_TEMPLATE

  Note: The parameter values below are ONLY supported on platforms interfacing to the Honeywell 6703/6603 scanner.
  See Also:
    Constant Field Values

### DEC_ILLUM_POWER_LEVEL

    public static final int DEC_ILLUM_POWER_LEVEL

  This parameter sets the level of illumination by altering laser/LED power. Power Level(1/2/3/4/5/6/7).
  See Also:
    Constant Field Values

### DEC_PICKLIST_AIM_DELAY

    public static final int DEC_PICKLIST_AIM_DELAY

  Note: The parameter values below are ONLY supported on platforms interfacing to the Honeywell 3680 scanner.
  See Also:
    Constant Field Values

### DEC_PICKLIST_AIM_MODE

    public static final int DEC_PICKLIST_AIM_MODE

  Note: The parameter values below are ONLY supported on platforms interfacing to the Honeywell 3680 scanner.
  See Also:
    Constant Field Values

### DOTCODE_ENABLE

    public static final int DOTCODE_ENABLE

  This property specifies whether Dotcode decoding is enabled.
  See Also:
    Constant Field Values

### DPM_DECODE_MODE

    public static final int DPM_DECODE_MODE

  This property specifies whether DPM decoding is enabled during the execution of Decode.
  See Also:
    Constant Field Values

### WEDGE_KEYBOARD_ENABLE

    public static final int WEDGE_KEYBOARD_ENABLE

  This property specifies whether Keyboard mode is enabled. If the configured PropertyID.WEDGE_KEYBOARD_ENABLE is 1, append the barcode text to TextBox, input method, or send the barcode text as key events.
  See Also:
    Constant Field Values

### WEDGE_KEYBOARD_TYPE

    public static final int WEDGE_KEYBOARD_TYPE

  This property specifies select an option for keystroke types. Values: 0 : Auto append text to TextBox. 1 : If there is no TextBox, append text to input method. 2 : Send key event. 3 : Auto append text to input method.
  See Also:
    Constant Field Values

### WEDGE_INTENT_ACTION_NAME

    public static final int WEDGE_INTENT_ACTION_NAME

  The intent action name is to receive barcode data. The default is "android.intent.ACTION_DECODE_DATA".

  See Also:
    ACTION_DECODE

### WEDGE_INTENT_LABEL_TYPE_TAG

    public static final int WEDGE_INTENT_LABEL_TYPE_TAG

  A string tag represents the barcode type. The default is "barcodeType".
  See Also:
    BARCODE_TYPE_TAG

### WEDGE_INTENT_DATA_STRING_TAG

    public static final int WEDGE_INTENT_DATA_STRING_TAG

  A string tag represents the barcode string. The default is "barcode_string".

  See Also:
    BARCODE_STRING_TAG

Constructor Detail

### PropertyID

    public PropertyID()

  This class contains all supported Scanner sub-system reader properties.